Introduction

|  |  |  |  |  |
| --- | --- | --- | --- | --- |
| |  |  | | --- | --- | |  | **APPROVED** |  |  | | --- | | Id.: AFM/NORM/GEN/00009222.0001001 / 14 Jan 15 Criteria: SA  Applicable to: MSN 6445, 6555  Applicable to: MSN 6445, 6555  Applicable to: 9N-AKW 9N-AKX | |  |   **INTRODUCTION**  The procedures contained in this chapter have been established and are recommended by the aircraft manufacturer.  Only particular operations which are considered useful to highlight are presented. The procedures which are considered to be "basic airmanship" are therefore not covered.  When actions depend on a condition, a dot (•) or a square (■) identifies this condition. The square is used when there is a choice between one or more conditions and only one is applicable.  These procedures are approved by the Airworthiness Authorities as acceptable procedures for a convenient use of the aircraft. This approval does not prevent the operator from developing equivalent procedures provided these procedures are approved by appropriate operational authorities.  // END |